



A screenshot of a computer

Description automatically generated



The baud rate is determined by how frequently **Timer 1 overflows**, and the overflow rate depends on how fast the 8051 processes machine cycles